A B C D E F G H I K L M N O P Q R S T U V W

## B

baBmpToSendData(int, Bitmap, BitmapToByteData.BmpType) - Static method in class net.posprinter.utils.BitmapToByteData
backFeed(int) - Static method in class net.posprinter.utils.DataForSendToPrinterTSC
  This command feeds the label in reverse.
BackgroundInit - Interface in net.posprinter.posprinterface
  The implementation method of this interface runs in the worker thread of the asynchronous task,and the normal execution is completed, returns true, otherwise false
bar(int, int, int, int) - Static method in class net.posprinter.utils.DataForSendToPrinterTSC
  This command draws a bar on the label format.
barCode(int, int, String, int, int, int, int, int, String) - Static method in class net.posprinter.utils.DataForSendToPrinterTSC
  This command prints 1D barcodes.
bitmap(int, int, int, Bitmap, BitmapToByteData.BmpType) - Static method in class net.posprinter.utils.DataForSendToPrinterTSC
  This command draws bitmap images (as opposed to BMP graphic files).
BitmapProcess - Class in net.posprinter.utils
  Image processing For printers, there are image processing: such as image rotation, reverse, mirror printing, etc., you can also directly process the image before printing
BitmapProcess() - Constructor for class net.posprinter.utils.BitmapProcess
BitmapToByteData - Class in net.posprinter.utils
  Covert bitmap to bytes
BitmapToByteData() - Constructor for class net.posprinter.utils.BitmapToByteData
BitmapToByteData.AlignType - Enum in net.posprinter.utils
BitmapToByteData.BmpType - Enum in net.posprinter.utils
blineBydot(int, int) - Static method in class net.posprinter.utils.DataForSendToPrinterTSC
  This command sets the height of the black line and the user-defined extra label feeding length each form feed takes.
blineByinch(double, double) - Static method in class net.posprinter.utils.DataForSendToPrinterTSC
  This command sets the height of the black line and the user-defined extra label feeding length each form feed takes.
blineBymm(double, double) - Static method in class net.posprinter.utils.DataForSendToPrinterTSC
  This command sets the height of the black line and the user-defined extra label feeding length each form feed takes.
blineDetect(int, int) - Static method in class net.posprinter.utils.DataForSendToPrinterTSC
  This command feeds the paper through the black mark sensor in an effort to determine the paper and black mark sizes, respectively.
block(int, int, int, int, String, int, int, int, int, int, String) - Static method in class net.posprinter.utils.DataForSendToPrinterTSC
  This command prints paragraph on label.
block(int, int, int, int, String, int, int, int, String) - Static method in class net.posprinter.utils.DataForSendToPrinterTSC
  This command prints paragraph on label.
box(int, int, int, int, int) - Static method in class net.posprinter.utils.DataForSendToPrinterTSC
  This command draws rectangles on the labe
BtPathName - Variable in class net.posprinter.service.PrinterConnectionsService.Printer
byteMerger(byte[], byte[]) - Static method in class net.posprinter.utils.PosSetting
byteMerger(byte[], byte[]) - Static method in class net.posprinter.utils.StringUtils
bytes2HexString(byte[]) - Static method in class net.posprinter.utils.StringUtils

A B C D E F G H I K L M N O P Q R S T U V W